Refo Yudhanto

CS350

HW 4

1. T
2. Check init if it can reach a looping SCC in graph G that contains yellow and blue node.